
Demonstrations for TIMH operation.This example code demonstrates how pwm waveform sync start with sync_PCI(SPCI).

1. pwm waveform sync start by using sync_PCI(SPCI).

2. sync_PCI(SPCI) of timh1 and timh2 configed bypass enable. And the bypass source config as timh0.
 
 
 !!More detail of the waveform please refer to : timh\sync_pci_SPCI\doc\
 
