Demonstrations for SPI master(Half-Duplex) communicating
with SPI slave through Interrupt modes.

Four lines communication:
	baudrate : 4000000
	data width : 8bit
	MSB first
	CS Pin Controlled by SPI module.