Demonstrations for LVD operation.
1. LVD1 low voltage reset demo : When VCC is lower than 3.20+0.05V/-0.05V, the chip will be reset.
2. LVD2 low voltage warning demo : When VCC is lower than 4.00+0.05V/-0.05V, will generate an interrupt.