Demonstrations for ADC operation.
Prepare requirements: (1)PD6 connects to slide rheostat, external voltage
supply, temperature sensor, etc.

1. ADC analog watchdog demo: ADC samples PD6's input, if the converted result
is bigger than the high threshold, it will trigger a compare event.


