Demonstrations for Basetimer operation.This example code demonstrates how Basetimer work in 16bit mode.
  

BTIM00, interrupts per a constante interval of 138.6ms. Toggle PA1(LED_S2).

BTIM01, interrupts per a constante interval of 418.6ms. Toggle PD12(LED_S3).


  
 
