Demonstrations for ADC operation.
Prepare requirements: (1)PD6 connects to slide rheostat, external voltage
supply, temperature sensor, etc.

1. ADC samples PD6's input, convert the result, using polling to get the result.


