
Demonstrations for WWDG  operation.

1.When feed dog LED SI will blink;
2.When WWDG arrived in time UART print "Wait for system reboot by WWDG.";
3.If successful wake up CPU, UART print "WWDG already reboot, test success.";